Power Plant Energy Predictions – Video Script.

This is our script.

|  |  |  |
| --- | --- | --- |
| Person | Script | Approx.  Duration |
|  | TITLE CARD: USD - MS AAI | 10s |
| Israel | We live in the era of information, the time when everyone is connected to the Internet 24/7, in our cell phones, in our computers. | 10s |
|  | TITLE CARD: AAI-500- Probability and Statistics for Artificial Intelligence. | 10s |
| Darin | It’s easy sometimes to take it for granted, we’re used to it. It’s sometimes hard to realize these things are there: a refrigerator or a microwave in our kitchen, our LED television, the light in our house, everything is just there for us, all the time. | 16s |
|  | TITLE CARD: Professor Dallin Munger, M.S. | 10s |
| Mani | We don’t even see it anymore. We only notice that it’s there when it’s gone: A power outage and then you notice, because NOTHING seems to work without it. | 11s |
| Israel | We’re obviously talking about electrical power. Without it, no battery charging for your cell phone. The food in the refrigerator will go bad, and the A/C wouldn’t run. | 12s |
| Darin | Without it, you couldn’t even watch this video. No video conferences, no video games. Electric power is everything. I cannot think of an industry that could live without it today. | 11s |
| Mani | Without it, the whole economy of the world would collapse. Electric power is as vital today as water or air and it has been for the past century. So, producing electricity is one of the most important tasks in the world. | 16s |
| Israel | There are many kinds of Power Plants: burning fuel, solar, Aeolic, geothermal, nuclear. But today we’re going to talk about Combined Cycle Power Plants. Have you heard about them? | 12s |
| Darin | Combined Cycle Power Plants, or CCPP for short, are more efficient because they combine multiple methods.  In the first Stage of the plant they burn fuel and make a turbine spin to induce electricity. That produces a lot of heat. | 17s |
| Mani | Typical fuel plants let that heat escape, but CCPP use that residual heat as the source input for Stage Two: they boil water and use the steam to make a second turbine spin, inducing even more electricity, releasing water vapor into the atmosphere. | 18s |
| Israel | It's a masterpiece of engineering in our time capable of delivering typically from 100 up to 1000 Megawatts per hour depending on the number of combustion turbines, steam turbines, and other optimized heat recovery systems. | 15s |
| Darin | CCPP’s are also impacted by weather factors, such as ambient temperature, atmospheric pressure, and relative humidity. These factors have a direct influence in the energy output of the power plants, which affects their efficiency and ultimately translates in economic gains or losses for the investors of the plant, and ultimately to the final user: all of us. | 25s |
| Mani | Can you imagine if we could know in advance the energy output of these power plants based on the atmospheric conditions?  What if we could input the information on the weather forecast to accurately predict the efficiency of the CCPP? | 17s |
|  | TITLE CARD: Team 2 Presents… | 10s |
| Israel | Imagine the impact of such forecast to the demand; the general public as well as companies could prepare in advance for their energy needs and make decisions to effectively plan their upcoming energy bill. I’m Israel Romero | 15s |
| Darin | I’m Darin Verduzco | 2s |
| Mani | I’m Manikandan Perumal, and together we’ll show you a model we built to effectively predict the output of a Combined Cycle Power Plant with more than 95% accuracy. | 12s |
|  | TITLE CARD: POWER PLANT ENERGY PREDICTIONS. | 10s |